                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3345098
Touch-Mi Ender 3 / CR10 Hotend FanDuct stock fan by fafabienman is licensed under the Creative Commons - Attribution - Non-Commercial - No Derivatives license.
http://creativecommons.org/licenses/by-nc-nd/3.0/

# Summary

Adaptation of HOTEND Ender 3 / CR10 fan duct.
 for Mi-Touch compatibility

You need :

- Kit Touch-Mi sensor (with wires and inox screw)
- M3 nut
- 2 screws


You can adjust the height of the Mi-Touch with the screw/nut 

For fix the fixed plate magnet on X axis i have use 2 screws in the free holes (i have dumper).

Be careful that if you print near X0 not to get too close the fixed magnet otherwise the PIN go down and risk to clash.

I recommand to print the Duct Fan in PETG or better : ABS.
PLA is only ok for the fix magnet

Orignal part : https://www.thingiverse.com/thing:2879538

If you like it ;)  
<table border="0" cellpadding="0" cellspacing="0" align="LEFT"><tbody><tr><td align="center"></td></tr><tr><td align="center"><a href="https://paypal.me/fafabienman" title="As you want :) Thx for me" onclick="javascript:window.open('https://paypal.me/fafabienman','WIPaypal','toolbar=no, location=no, directories=no, status=no, menubar=no, scrollbars=yes, resizable=yes, width=1060, height=700'); return false;"><img src="https://www.paypalobjects.com/webstatic/mktg/logo/pp_cc_mark_37x23.jpg" border="0" alt="PayPal Logo" /></a></td></tr></tbody></table>

# Print Settings

Printer Brand: Creality
Printer: Ender 3
Rafts: No
Supports: No
Resolution: 0.2
Infill: 15
Filament_brand: Amazon Basics
Filament_color: Black
Filament_material: PETG